<?xml version="1.0" encoding="utf-8" standalone="yes"?>

<?xml-stylesheet href="./_c74_ref.xsl" type="text/xsl"?>

<!--This is an automatically generated file. DO NOT EDIT THIS FILE DIRECTLY. Rather, use the _ref.xml files found in the 'edits' folder.-->
<c74object name="el.clean_gate~">
	<digest>
		<o>el.clean_selector~</o> Gate with cross-fade for smooth transitions.
	</digest>
	<description>
		This object is like gate~ except that it crossfades between the signals. Output channels are counted starting from 1. When the output channel is set to 0, the gate is closed. This output channel may be set with either integer input, or signal input. With signal input, the response of el.clean_gate~ is sample-accurate.
    </description>
	<!--METADATA-->
	<metadatalist>
		<metadata name="author">
			Eric Lyon
		</metadata>
		<metadata name="tag">
			MSP
		</metadata>
		<metadata name="tag">
			LyonPotpourri
		</metadata>
	</metadatalist>
	<!--INLETS-->
	<inletlist>
	</inletlist>
	<!--OUTLETS-->
	<outletlist>
	</outletlist>
	<!--ARGUMENTS-->
	<objarglist>
		<objarg name="outlet count" type="int" optional="0">
			<digest>
				TEXT_HERE
			</digest>
			<description>
				The number of signal outputs.
			</description>
		</objarg>
		<objarg name="crossfade duration" type="float" optional="0">
			<digest>
				TEXT_HERE
			</digest>
			<description>
				Cross fade duration in milliseconds.
			</description>
		</objarg>
	</objarglist>
	<!--MESSAGES-->
	<methodlist>
		<method name="fadetime">
			<arglist>
                <arg name="channel number" type="float" optional="0" id="1" />
                
			</arglist>
			<digest>
				TEXT_HERE
			</digest>
			<description>
				Set the fade time in milliseconds.
			</description>
		</method>

	</methodlist>
	<!--ATTRIBUTES-->
	<attributelist>
	</attributelist>
	<!--SEEALSO-->
	<seealsolist>
		<seealso name="gate~"/>
        <seealso name="clean_selector~"/>
	</seealsolist>
    
</c74object>
